

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Type | Size | | Accuracy  (mV/Pa) | | polarizing voltage; (V) | | Frequency  range(Hz) | | frequency response characteristics | dynamic range (dB) \* | | electric capacity(pF) | | Temperature coefficient(dB/℃) | | Size | | Characteristic |
| 14405 | | Φ6.35 mm (1/4") | | 3.5 | | 10～70,000 | | Free field | | | 40～160 | | 6.5 | | WS3型 | | Wide range of frequency and loud soud | |
| 14406 | | 2.5 | | 10～40,000 | | Sound pressure | | | 40～160 | |
|  | |  | |  | |  | |  | | |  | |  | |  | |  | |